{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":3,"n_cols":6,"rows_kept":3,"merged":[[0,0,0,5]],"flags":["formulas_cached_only"]}
["爱店海关手持式核素识别仪装备需求清单"]
["序号","品名","数量","单价预算（元）","技术指标","备注"]
[1,"手持式核素识别仪",1,81390,"1.探测器：Ф50×50mmNaI(TI)+能量补偿型GM管\n2.显示屏：≥3.2寸，分辨率≥320×240 彩屏\n3. 测量模式：采样识别、剂量、剂量率、寻源\n4. 灵敏度：≥2000cps（137 Cs，1μGy/h）\n5. 能量范围：30KeV~3MeV\n6. 剂量当量率范围：0.01μSv/h ~100mSv/h\n7.累积剂量范围：0~9999 mSv\n8.分辨率：（@ 661keV）7%（NaI）\n9. 置信度：≥95%\n10.相对固有误差：剂量当量率：≤±20%，剂量当量：≤±15%\n11.变异系数：≤15%\n12.入射角响应：2π立体角的响应变化≤20%\n13.放射性核素识别种类：\n特殊核材料：233U、235U、238U、237U、239U\n医用核材料：18F、67Ga、99mTc、111In、153Sm、123I、125I、131I、133Xe、201TI、51Cr、103Pd\n工业用核素：57Co、75Se、60Co、133Ba、137Cs、192Ir、241Am、152Eu\n天然核素：40K、226Ra、232Th、238U\n14. 核素识别率及识别时间：单核素：≥95%，≤1min；多核素：≥95%，≤2min\n15. 能谱特征：≥2048道，线性，校准和稳定化能量刻度\n16.图谱存储：可存储5000组以上图谱数据\n17. 核素库：内置核素库，可学习并自定义核素库\n18. 工具软件：自带上位机数据管理软件、谱分析软件\n19.报警方式：声、光报警\n20. 响应时间：≤10s\n21. 供电：内置充电锂电池\n22.工作时间：≥ 8h\n23.温度监控：内置温度传感器，可显示当前温度\n24.工作温度：-30℃～+50℃\n25. 贮存温度：-40℃～+55℃\n26.相对湿度：≤95% (35℃，非冷凝)\n27.防护等级：≥ IP56\n28.重量：≤2.5kg","①不得超过单价预算；②性能需满足或优于技术指标。"]