{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":5,"n_cols":7,"rows_kept":5,"merged":[[0,0,0,6]],"flags":["formulas_cached_only"]}
["玉林海关气体检测设备需求清单"]
["序号","品名","数量","单价预算（元）","功能概述","主要技术指标","备注"]
[1,"溴甲烷浓度检测仪",1,20000,"熏蒸散气后检测溴甲烷的残留量等。","1.测量量程：0-1000ppm(溴甲烷)；\n2.分辨率：0.01ppm；\n3.检测精度：≤±lppm(溴甲烷)；\n4.环境温度：-10℃-40℃；\n5.环境湿度：5-90%RH；\n6.传感器：高精度光声光谱传感器；\n7.报警方式：具有视觉、振动和声音（95分贝）；\n8.报警等级：低、高、STEL、TWA、OL（超量程）；\n9.电池：可充电电池，可连续工作8小时；\n10.CNAS认可的第三方检测机构出具的浓度检测测试报告；\n11.显示屏：彩色显示屏，支持ppm和g/m3浓度单位切换。","设备需在合同签订后7日内在广西玉林市交付采购人。"]
[2,"便携式三合一熏蒸气体红外检测仪",1,50000,"用于熏蒸过程中熏蒸气体浓度检测","1.检测气体：硫酰氟、溴甲烷、磷化氢\n★2.检测量程：硫酰氟（0-200 g/m3）、溴甲烷（0-200 g/m3）、磷化氢（0-2000ppm）；\n3.检测原理：红外NDIR；\n4.检测精度：±1% FS；\n5.分辨率：0.1g/m3、1ppm；\n▲6.高清彩屏,可同时显示硫酰氟、溴甲烷、磷化氢气体浓度值；\n▲7.红外气体分析仪数据采集软件：提供“红外气体分析仪数据采集软件”软件著作权登记证书；\n▲8.仪器内置流量传感器，分析仪屏幕显示采样流量；\n9.分析仪开机预热界面显示预热进度；\n10.分析仪测量界面显示环境温度和环境压力；\n11.分析仪前后两端带散热格栅；\n12.分析仪测量状态可开启和关闭报警声音；\n13.分析仪在测量状态下可手动进入吹扫模式，吹扫结束后气泵关闭，分析仪进入待检模式；\n14.（配备上位机软件，可自定义配置设备的（如气体单位、报警限值等）功能参数；\n15.可设置开机自动校准零点，也可手动按需进行零点校准；\n16.仪器在检测过程中连续工作，无需定期通入新鲜空气；\n17.仪器具备数据存储功能，可通过U盘导出数据；\n18.工作温度：5~40℃；\n19.相对湿度：0~95%RH 非冷凝。","设备需在合同签订后7日内在广西玉林市交付采购人。"]
[3,"手持式熏蒸气体检测仪",2,5000,"用于各类磷化氢气体的检测","1.测量范围：0-20PPM；\n2.标准气体及浓度：磷化氢 10PPM；\n3.示值误差：≤±3%；\n4.响应时间:≤30S。","设备需在合同签订后7日内在广西玉林市交付采购人。"]