{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":13,"n_cols":6,"rows_kept":13,"merged":[[0,0,0,5]],"flags":["formulas_cached_only"]}
["凭祥海关仪器设备检定校准服务项目采购需求"]
["序号","设备名称","型号","数量","检定校准周期","校准标准"]
[1,"手持式核素识别设备","中检维康NCR31",2,"1次/年","《用于探测与识别放射性核素的手持式辐射监测仪校准规范》"]
[2,"手持式核素识别仪","identiFINDER2-NG",1,"1次/年","《用于探测与识别放射性核素的手持式辐射监测仪校准规范》"]
[3,"手持式体温快速筛查仪","TE-W400",4,"1次/年","《测量人体温度的红外温度计校准规范》"]
[4,"行人放射性监测系统","RM1000NH",1,"1次/年","《行人与行李放射性监测装置校准规范》"]
[5,"入境行人核辐射监测系统","PR400",1,"1次/年","《行人与行李放射性监测装置校准规范》"]
[6,"红外筛检仪","F2123-T",4,"1次/年","《测量人体温度的红外温度计校准规范》"]
[7,"水银体温计","无",10,"1次/年","JJG881-1994《标准体温计》"]
[8,"远程智能检测终端","中海科YZJ-4",1,"1次/年","《测量人体温度的红外温度计校准规范》"]
[9,"口岸卫检智慧通道","SQIS2110",1,"1次/年","《测量人体温度的红外温度计校准规范》"]
[10,"零公里处核辐射探测门","G3910-8200",1,"1次/年","《通道式车辆放射性监测系统校准规范》"]
[null,null,"合计",26]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}